Wave

A versatile DOS/Windows format using the RIFF format (chunk id is Wave). Wave supports a huge number of sub-formats, many of which are proprietary compression algorithms and information is not available. Some others not listed below are MPEG, GSM and G72x.

Filetype | &FB1 (Wave)
Channels | Any (only plays mono/stereo)
Rates | Any
Subformats | 8-bit unsigned linear
| 16-bit signed linear
| 8-bit µ-law
| 8-bit A-law
| 4-bit Microsoft ADPCM
| n-bit IMA/DVI/Intel ADPCM (2-4 supported)
Annotation | All fields available

[ Parent ] [ Manual root ]